V2.0 Build0702

QGNSS V2.0 has undergone architecture upgrades compared to QGNSS V1.x:
1. Key functional modules and underlying protocol analysis:
① Firmware Download and NTRIP use process calls.
② QGNSSLog is embedded in QGNSS to support real-time playback and log playback through the database
③ Data analysis calls QGMI analysis library to achieve protocol differentiation and analysis.
2. Restructured the project structure to improve scalability.
3. Adopted standard module spelling.
4. Removed Text Data, Binary Data,and Unparsed Data views and added QConsole super debugging tool.
5. Unified window properties as sub-windows.

New features:
1. Added Ntrip Server and Caster functions
2. Added QConsole super debugging tool
3. Added real-time QGNSSLog display
4. Added Vertical View in Signal View
5. Added playback control shortcut bar in the status bar
6. Added Dashboard View interface to display speed, knots, altitude and heading.

Function optimization:
1. Optimized the QGNSSLog curve display to curve plus scattered points for representation

NOTE:
1. The path of QGNSS V2.0 should be concise, not exceeding 20 characters, to avoid interference with the firmware upgrade process. 
2. QGNSS V2.0 does not support the firmware upgrade of the modules or EVB listed below.  For update the firmware on those modules or EVB, please revert to QGNS V1.x.
① Module: L76, L76-L, LG77L (C), L26, L86, L96, L70-R, L80-R, LC79D series, LUA600A (00) and LUA300C (00)
② EVB: GNSS MODULE EVB 
3. If QGNSS V1.x is required, please contact Quectel Technical Support.